|  |  |  |
| --- | --- | --- |
| Model no  | YS1008-K-G-C13-U | 1.0U 8\*C13 outlets with anti-off locking, with switch,overload protection,USB charge |
|  |
| 10 | Spare parts | Mounting screw and nut 4sets, Installation Mannual | 11 | Rated current | 13A |
| 9 | Function | Overload protection，switch，5V2.1AUSB | 12 | Rated voltage | 250V |
| 8 | Plug | BS plug | CustomerATTN | Ismet C Soy | Customerapproval |  |
| 7 | Socket | 8\* C13 with anti-off locking |
| 6 | Connection box | none | Customer | Chronos Network Telecom.Consulting |
| 5 | Cable spec | 3\*1.5mm2\*2metre |
| 4 | Installation | 25+25mm mounting hook 180° horizontal |  |  |  |  |
| 3 | Mounting distance | 461±3mm |  |  |  |  |
| 2 | Product size | 483\*44.8\*45mm | Date | Engineer | Scale |  |  |
| 1 | Housing Material | Black 1.5U Aluminium, 45mm high | 2021.4.9 | Lee | 1.1 |  |  |