|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Model no | | YS1008-K-G-C13-U | | 1.0U 8\*C13 outlets with anti-off locking, with switch,overload protection,USB charge | | | | | | | |
|  | | | | | | | | | | | |
| 10 | Spare parts | | Mounting screw and nut 4sets, Installation Mannual | | 11 | Rated current | | 13A | | | |
| 9 | Function | | Overload protection，switch，5V2.1AUSB | | 12 | Rated voltage | | 250V | | | |
| 8 | Plug | | BS plug | | Customer  ATTN | Ismet C Soy | | Customer  approval | | |  |
| 7 | Socket | | 8\* C13 with anti-off locking | |
| 6 | Connection box | | none | | Customer | Chronos Network Telecom.Consulting | | | | | |
| 5 | Cable spec | | 3\*1.5mm2\*2metre | |
| 4 | Installation | | 25+25mm mounting hook 180° horizontal | |  |  | | |  |  | |
| 3 | Mounting distance | | 461±3mm | |  |  | | |  |  | |
| 2 | Product size | | 483\*44.8\*45mm | | Date | Engineer | Scale | |  |  | |
| 1 | Housing Material | | Black 1.5U Aluminium, 45mm high | | 2021.4.9 | Lee | 1.1 | |  |  | |